How to Install PCtel HSP Modems on Windows 2000

Contents:
	i.   PnP/PCI modem installation
	ii.  Install PnP/PCI modem Driver manually.

i. PnP/PCI modem installation

    
    Plug your modem(ISA PNP modem or PCI modem) into a free slot of
your computer and turn the power on, you may receive a message that
Windows 2000 has detected your Plug and Play device(s).

    When the modem has been detected, use the following steps:

    1. Press "Next" button when the "Upgrade Device Driver Wizard" 
       window appears.

    2. Select "Search for a suitable driver for my device [recommended]" 
       option and then press "Next" button.

    3. Insert ASUS Support CD to CD-ROM.

    4. Select "Specify a location" option and then press "Next" button.

    5. Type or browse the path {CD-ROM Drive}:\Modem\AMR\Win2K from 
       ASUS Support CD.

    6. Finally, follow the instruction to complete the installation.

Note:
    If Windows 2000 does not copy files during the installation, please
goto "Windows 2000/Inf" directory and delete unused "oem*.inf" and "oem*.pnf"
files, then try again.


ii. Install PnP/PCI modem Driver manually.

    1. Press "Start" button.

    2. Move highlight bar to "Settings" and select "Control Panel".

    3. Double click on "System" icon.

    4. Select "Hardware" page and then click [Device Manager] button.

    5. View device by type and find "Other devices" node.
   
    4. Right Click the "Software Modem" node.

    5. When the menu appears, click the "Properties" item.

    6. Please select [General] page to reinstall driver or select [Driver] 
       page to update driver.

    7. Press "Next" button when the "Upgrade Device Driver Wizard" window 
       appears.

    8. Select "Search for a suitable driver for my device [recommended]" 
       option and then press "Next" button.

    9. Insert ASUS Support CD to CD-ROM.

   10. Select "Specify a location" option and then press "Next" button.

   11. Type or browse the path {CD-ROM Drive}:\Modem\AMR\Win2K from ASUS 
       Support CD.

   12. Finally, follow the instruction to complete the installation.