How to Install PCtel HSP Modems on Windows 9X

Contents:
	i.   PnP/PCI modem installation
	ii.  Install PnP/PCI modem Driver manually

i. PnP/PCI modem installation

    Plug your modem(ISA PNP modem or PCI modem) into a free slot of
your computer and turn the power on, you may receive a message that
Windows 9X has detected your Plug and Play device(s).

    When the modem has been detected, use the following steps:

    1. Press Next while the "Update Device Driver Wizard" window appears.

    2. Select "Search for a better driver than the one your device is 
       using now.(Recommendation)" option and then press Next.

    3. Choose "Specify a location" check box. Type or browse the path 
       {CD-ROM Drive}:\Modem\AMR\Win9X to the driver and then press Next.

    4. Windows will then find the device "ASUS MR Series". Now you can 
       press Next to install the driver.

    5. Finally, press Finish to complete the installation.

ii.  Install PnP/PCI modem Driver manually

    1. Right-click "My Computer" icon from the desktop. Select "Properties" 
       item while the menu appears.

       or you can press "Start" button and move highlight bar to "Settings" 
       and select "Control Panel". Double click on "System" icon.

    2. Select "Device Manager" page.

    3. View device by type and find "Other devices" node.
   
    4. Select the "PCI Communication Device" node and then click the 
       "Properties" button.

    5. Select [General] page to reinstall driver or Select [Driver] page to 
       update driver.

    6. Press Next while the "Update Device Driver Wizard" window appears.

    7. Select "Search for a better driver than the one your device is using 
       now.(Recommendation)" option and then press Next.

    8. Choose "Specify a location" check box. Type or browse the path 
       {CD-ROM Drive}:\Modem\AMR\Win9X to the driver and then press Next.

    9. Windows will then find the device "ASUS MR Series". Now you can press 
       Next to install the driver.

   10. Finally, press Finish to complete the installation.