United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
System
Power supply
Diskette drive
Hard drives
DVD drive
CD drives
Mouse
Fax/modem
Zip drive
l
| SPECIFICATIONS Specifications for Quantum hard drives immediately follow this link to Seagate hard drives
Quantum Hard Drives
| 4.0-GB | 6.0-GB | 6.0-GB | 8.0-GB
Compaq Part Number | 286119 | 286122 | 286556 | 286123
Formatted Capacity |  |  |  |
Physical (MB) Logical (MB) | 4018 4018 | 6506 6506 | 6028 6028 | 8038 8038
Drive Type | 65 | 65 | 65 | 65
Transfer Rate |  |  |  |
Media (Mbits/sec) Interface (MBytes/sec) | 141.7 33.3 | 106.8 16.7 | 141.7 33.3 | 141.7 33.3
Typical Seek Time (including settling) |  |  |  |
Single Track (ms) Average (ms) Full Stroke (ms) | 2.5 12.0 24.0 | 1.1 11.0 18.0 | 2.5 12.0 24.0 | 2.5 12.0 24.0
Disk Rotational Speed (RPM) | 4000 | 4490 | 4000 | 4000
Cylinders |  |  |  |
Physical Logical | 11490 8306 | 7855 13446 | 11490 12459 | 11490 15574
Data Heads |  |  |  |
Physical Logical | 2 15 | 8 15 | 3 15 | 4 16
Sectors per Track |  |  |  |
Physical Logical | 261-403 63 | 149-269 63 | 261-403 63 | 261-403 63
Buffer Size (kB) | 128 | 128 | 128 | 128
Seagate Hard Drives
| 3.2 GB | 4.0-GB | 6.4 GB | 8.4 GB
Compaq Part Number | 262477 | 286118 | 179127 | 334180
Formatted Capacity |  |  |  |
Physical (MB) Logical (MB) | 3227.1 3227.1 | 4019 4019 | 6448.6 6448.6 | 8445.0 8445.0
Drive Type | 65 | 65 | 65 | 65
Transfer Rate |  |  |  |
Media (Mbits/sec) Interface (MBytes/sec) | 87.8 16.7 (non-UDMA) 33.0 (UDMA) | 87.8 16.7 | 83-140 33.3 | 83-140 33.3
Typical Seek Time (including settling) |  |  |  |
Single Track (ms) Average (ms) Full Stroke (ms) | 2.0 12.0 20.0 | 2.0 12.0 21.0 | 1.7 11.5 20.2 | 1.7 11.5 20.2
Disk Rotational Speed (RPM) | 4500 | 4500 | 5400 | 5400
Cylinders |  |  |  |
Physical Logical | 5690 6253 | 5690 7787 | 13328 8557 | 8557 16383
Data Heads |  |  |  |
Physical Logical | 6 16 | 8 16 | 6 15 | 8 16
Sectors per Track |  |  |  |
Physical Logical | 63 | 114-234 63 | 180-306 63 | 180-306 63
Buffer Size (kB) | 128 | 128 | 128 | 128
privacy and legal statement