United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
TROUBLESHOOTING Clearing CMOS 2nd Alternative Board for 5000/5100 Series Back to main page for 5000/5100 series
5 | To disable the password, move the jumper JP2 from pins 1-2 to pins 2-3 for 10 seconds, then return to pins 1-2.
6 | Replace the system board bracket and perform the desired troubleshooting.
| CMOS jumper location
Revised: 28 August 1998