United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
System
Power supply
Diskette drive
Hard drives
DVD drive
CD drives
Mouse
Fax/modem
Zip drive
l
| SPECIFICATIONS
DVD Drive
Dimensions | U. S. | Metric
Width Height Depth | 5.74 in 1.68 in 8.23 in | 14.60 cm 4.29 cm 20.80 cm
Weight | 1.80 lb | 0.9 kg
Applicable Disc |
DVD-5, DVD-9, DVD-10, DVD-18 CD-ROM CD-DA CD-XA Photo CD CD-I Ready CD-Bridge CD-R | Mode 1 and Mode 2 Audio Mode 2, Form 1 and 2 Single and Multiple Session
Block Size |
CD-ROM Mode 0 CD-ROM Mode 1 CD-ROM Mode 2 DVD | 2352 bytes 2352, 2340,2336, 2048 bytes 2352,2340, 2336, 2048 bytes 2048 bytes
Center Hole | 15 mm diameter
Diameter | 12 cm, 8 cm
Thickness | 1.2 mm
Track Pitch | 1.6 µm
Laser |
Beam Divergence Output Power Type Wave Length | 53.5 degrees +/- 1.5 degrees 5 mW Semiconductor laser GaAIAs 650 nm +/- 25 nm (DVD) 795 nm +/- 25 nm (CD)
Access Time |  |
Random Full Stroke | DVD: < 150 ms < 225 ms | CD: < 100 ms < 225 ms
Audio Output Level |
Line Out Headphone | 1.0 V (RMS) at 47 kW 0.7 V (RMS) at 32 W
Cache Buffer | 128 kB
Sustained Data Transfer Rate | 150 KB/sec (single, CD-ROM mode) 1200-3000 KB/sec (20× CAV CD-ROM mode) 2760 KB/sec (DVD mode)
Interface Cable Length (Max) | 18 in
Startup Time | < 15 sec
Stop Time | < 2 sec
privacy and legal statement