United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
Processor & goalposts
Memory module
Video memory
Battery
System board
Heat sink clip
I-O panel
System board components index page
l
| REMOVAL & REPLACEMENT System Board Components Processor - 4900 Series
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
4 | Open the system board bracket
5 | Locate the AMD K6 processor
6 | Remove the clip from the heat sink
7 | Lift up the ZIF socket handle and lift the heat sink and processor out of the socket
To reinstall the AMD K6 processor, rub a thermal transfer crayon on the bottom of the heatsink, then reverse the steps above. (The thermal transfer crayon replaces the thermal pad used with earlier K6 processors.)
privacy and legal statement