United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic discharge
Service considerations
Preparation for disassembly
Serial number
Hood
Fax-modem
System board bracket
Serial port assembly
Mass storage devices
System board
Power supply
Front bezel
Instant On button board
Creativity Action Center
| REMOVAL & REPLACEMENT Fax/modem
1
| Perform preparation procedures.
2 | Remove the hood.
3 | Remove the screw holding the fax/modem bracket to the chassis and pull the fax/modem out of the slot.
To replace the fax/modem, reverse this procedure.
IMPORTANT: | When replacing the fax/modem, download the latest software from SoftPaq. If QuickRestore is used, it may not have the 56K upgrade software included.

privacy and legal statement