United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
System
Power supply
Diskette drive
Hard drives
DVD drive
CD drives
Mouse
Fax/modem
Zip drive
l
| SPECIFICATIONS CD Drives Information for the 32x CD drive immediately follows this link to the 24x CD drive
32× CD Drive
Dimensions | U. S. | Metric
Width Height Depth | 5.75 in 1.67 in 8.23 in | 14.80 cm 4.20 cm 20.80 cm
Weight | 2.65 lb | 1.2 kg
Applicable Disc |
CD-ROM CD-DA CD-XA Photo CD | Mode 1 and Mode 2 Audio Mode 2, Form 1 and 2 Single and Multiple Session
Block Size |
CD-ROM Mode 1 CD-ROM Mode 2 CD-DA CD-XA | 2048 bytes 2340, 2336 bytes 2352 bytes 2328 bytes
Center Hole | 15 mm diameter
Diameter | 12 cm, 8 cm
Thickness | 1.2 mm
Track Pitch | 1.6 µm
Laser |
Beam Divergence Output Power Type Wave Length | 53.5 degrees +/- 1.5 degrees 0.14 mW Semiconductor laser GaAIAs 780 nm +/- 25 nm
Access Time |
Random Full Stroke | < 85 ms < 145 ms
Audio Output Level |
Line Out Headphone | 0.8 V (RMS) at 10 kW 0.6 V (RMS) at 32 W
Cache Buffer | 256 KB
Data Transfer Rate |  |
Sustained Burst | Mode 1 2062 KB/sec (single) 4800 KB/sec (32×) 16.7 MB/sec | Mode 2 2368 KB/sec (single) 5512 KB/sec (32×) 16.7 MB/sec
Interface Cable Length (Max) | 18 in
Startup Time | < 7 sec
Stop Time | < 4 sec
24× CD Drive
Dimensions | U. S. | Metric
Width Height Depth | 5.75 in 1.67 in 8.23 in | 14.60 cm 4.29 cm 20.80 cm
Weight | 1.98 lb | 0.95 kg
Applicable Disc |  |
CD-ROM CD-DA CD-XA Photo CD | Mode 1 and Mode 2 Audio Mode 2, Form 1 and 2 Single and Multiple Session
Block Size |
CD-ROM Mode 1 CD-ROM Mode 2 CD-DA CD-XA | 2048 bytes 2340, 2336 bytes 2352 bytes 2328 bytes
Center Hole | 15 mm diameter
Diameter | 12 cm, 8 cm
Thickness | 1.2 mm
Track Pitch | 1.6 µm
Laser |
Beam Divergence Output Power Type Wave Length | 53.5 degrees +/- 1.5 degrees 0.14 mW Semiconductor laser GaAIAs 780 nm +/- 25 nm
Access Time |
Random Full Stroke | < 85 ms < 150 ms
Audio Output Level |
Line Out Headphone | 0.8 V (RMS) at 47 kW 0.6 V (RMS) at 32 W
Cache Buffer | 128 KB
Data Transfer Rate |
Sustained Burst | 150 KB/sec (single) 3600 KB/sec (24×) 4.0 MB/sec
Interface Cable Length (Max) | 18 in
Startup Time | < 7 sec
Stop Time | < 4 sec
privacy and legal statement