United States
Maintenance and Service Guide Compaq Presario 7300 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
CPU Jumper Setting Table (Switch 1)
JUMPER & SWITCH INFORMATION
CPU | SDRAM | PCI | 1 | 2 | 3 | 4
66.8 | 66.8 | 33.4 | on | on | on | off
75 | 75 | 30 | off | on | on | off
83.3 | 83.3 | 33.3 | on | off | on | off
95 | 95 | 31.7 | off | off | on | off
100 | 100 | 33.4 | on | on | off | off
112 | 112 | 37.3 | off | on | off | off
124 | 124 | 31 | on | off | off | off
133 | 133 | 33.3 | off | off | off | off
90 | 90 | 30 | on | on | on | on
83 | 55.5 | 33.3 | off | on | on | on
95 | 63.3 | 31.7 | on | off | on | on
66.8 | 100 | 33.3 | off | off | on | on
105 | 105 | 35 | on | on | off | on
112 | 74.7 | 37.3 | off | on | off | on
124 | 82.7 | 31 | on | off | off | on
133.3 | 88.9 | 33.3 | off | off | off | on
| CAUTION: It is strongly recommended that the system speed is set according to the hardware configuration: CPU, SDRAM, Cards, etc.
Top of Page
Revised: 30 October 1998