United States
Maintenance and Service Guide Compaq Presario 7300 Series Computers
| Product Description | Troubleshooting | Illustrated Parts Catalog
Home | Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic Discharge
Preparation for Disassembly
Service Considerations
Serial Number
Chassis Cover
Fax-Modem
Mass Storage Devices
System Board and Components
Power Supply
> | REMOVAL & REPLACEMENT Service Considerations Tool Requirements Phillips screwdriver Needle-nose pliers Flathead screwdriver Compaq Utilities software Screws The screws used in these products are not interchangeable. If an incorrect screw is used during the reassembly process, it could cause damage to the unit. Compaq strongly recommends that all screws removed during the disassembly process be kept with the part that was removed, then returned to their proper locations.
> IMPORTANT: | As each subassembly is removed from the computer, it should be placed away from the work area to prevent damage.
> Cables and Connectors Most cables used throughout the unit are ribbon cables. These must be handled with extreme care to avoid damage. Apply only the tension required to seat or unseat the cables during insertion or removal from the connector. Handle cables by the connector whenever possible. In all cases, avoid bending, twisting, or tearing the cables, and ensure that they are placed in such a way that they cannot be caught or snagged by parts being removed or replaced.
> | CAUTION: When servicing these computers, ensure that cables are placed in their proper location during the reassembly process. Improper cable placement can cause severe damage to the unit.
Ribbon Cable Positions |
CD Drive | Hard Drive
Diskette drive | Button Board |
Power Supply |  |
privacy and legal statement