mls_prefix sbos_error

sbos_error 1 Not Enough DRAM on the InterWave to Run IWSBOS in DRAM Mode $
sbos_error 2 Bad or Missing IWSBOS Library File $
sbos_error 3 Invalid Selection for MPU-401 Base Port Address in IW.INI $
sbos_error 4 Invalid Selection for ROM Bank in IW.INI $
sbos_error 5 Invalid Selection for IWSBOS Communication Vector in IW.INI $
sbos_error 7 Can't Read CSN= or PNPRDP= from [setup 0] in IW.INI $
sbos_error 10 Can't Find InterWave Card $
sbos_error 11 The InterWave Hardware is Currently In Use by Another Device $
sbos_error 13 Cannot Load - Another InterWave TSR is Currently Using Hardware$

sbos_error 50 InterWave SBOS Version $

sbos_error 100 IWSBOS Driver Not Loaded

sbos_error 101 
Can't Unload IWSBOS While Windows is Running!
Exit Windows, then type 'IWSBOS /f' to unload

sbos_error 102 Initializing IWSBOS to run in Windows DOS BOX!
sbos_error 103 IWSBOS Can Not Gain Access to the Windows Drivers!
Check That VIWD.386 is Properly Loaded in SYSTEM.INI.
Emulation is Not Available Under Windows.

sbos_error 104 Cant find the INTERWAVE environment variable
sbos_error 106 Version number mismatch
Driver should be reinstalled

sbos_error 107 InterWave SBOS Loader Version
sbos_error 108 IWSBOS: Driver data space has an invalid size.
Driver should be reinstalled

sbos_error 109 Invalid Base Port Selection - Cannot load IWSBOS!
sbos_error 110 No resources allocated to SB emulation.
SB DAC emulation deactivated.

sbos_error 111 Invalid IWSBOS Interrupt Selection
sbos_error 112 Invalid InterWave Interrupt Selection
sbos_error 113 The InterWave Hardware is Currently in Use by Another Device
sbos_error 114 InterWave Card Not Found
sbos_error 115 Timer Vector has been Hooked
sbos_error 116 Keyboard Vector has been Hooked
sbos_error 117 DOS Multiplexed Interrupt has been Hooked
sbos_error 118 DOS Vector has been Hooked
sbos_error 119 Cannot Unload IWSBOS
sbos_error 120 IWSBOS resides at too deep of a directory structure to load
Move the IWSBOS executables to a higher level and try to load again

sbos_error 121 Memory control block destroyed
sbos_error 122 Unable To Free Device Driver
sbos_error 123 IWSBOS Driver Freed
sbos_error 124 The NMI procedure cannot be changed on this P.C.
sbos_error 125 The NMI procedure on this P.C. is disabled.
sbos_error 126 The InterWave Port Address is in Conflict
sbos_error 127 The NMI is not functioning on the InterWave
sbos_error 128 Can't Open Library File
sbos_error 129 Invalid Library Header
sbos_error 130 IWSBOS: Library version does not match driver's.
IWSBOS: Data may not be valid

sbos_error 131 Can't Read Data From Library File
sbos_error 132 Can't Allocate Download Buffer
sbos_error 133 No IWSBOS Data Found in ROMs

sbos_error 134
IWSBOS [[/opt1] [/opt2] ... ]
        /MPU401    Enable MPU-401 Emulation mode\n");
        /QUIET     Don't display banner messages when loading\n");
        /A         Turn off SoundBlaster DAC emulation\n");
        /C         Don't use NMI for emulation\n");
        /F         Remove the resident driver from memory\n");
        /V[D][F]   Set the Maximum volume for FM and/or Digital playback\n");
                   - VD - Set max. digital attenuation (0-N)\n");
                   - VF - Set max. FM attenuation (0-64)\n");
                   (Higher numbers means quieter playback)\n");
        /? or /H   Print this message\n");
	
sbos_error 135 Copyright (C) 1992, 1995 Advanced Gravis, Inc. All Rights Reserved.
