mls_prefix iwinit_message

#USAGE_MESSAGE
iwinit_message 1
USAGE: iwinit [options]
      ID=XXXXXX		vendor id for sound card
      INTERWAVE=X:\XXX	path & filename of configuration file. (.SYS driver)
      -q[X]   quiet [X = 1: Error Messages Only; X = 2: No Messages]
      -v[Y]   verbose [Y = 1..9; Verbosity level, 9 = Most Verbose]

#COPYRIGHT_MESSAGE
iwinit_message 2
InterWave Initialization Version 1.13

#PNP_BIOS_FOUND
iwinit_message 3
Found a Plug And Play BIOS.

#PNP_CM_FOUND
iwinit_message 4
Found a Plug And Play Configuration Manager.

#BAD_PNP_BIOS_HEADER
iwinit_message 5
Plug And Play BIOS Detected BUT Header Structure Was Bad.

#PNP_ISA_CONFIG_ERROR
iwinit_message 6
WARNING: could not get PnP ISA Configuration Structure. Code: %xh\n

#ERROR_WRITING_PROFILE
iwinit_message 7
Could not write PnP information to configuration file.

#IW_INITED
iwinit_message 8
InterWave card #%d initialized.

#FOUND_DRAM
iwinit_message 9
Found %ld bytes of DRAM.

#FOUND_ROM
iwinit_message 10
Found ROM chip: %s.

#NO_IW_CARDS_FOUND
iwinit_message 11
No InterWave Cards Were Found.

#NO_CM_NO_IW_PNP
iwinit_message 12
WARNING:
There are two or more Plug-and-Play cards in this computer.  No 
Configuration Manager was detected.  To gurantee there are no
resource conflicts between the add-on cards in this computer,
a Plug-and-Play Configuration Manager should be installed.

#NO_LEGACY_TO_CONFIG
iwinit_message 13
There are no legacy mode InterWave cards defined in the configuration file.

#INSUFFICIENT_LEGACY_DATA
iwinit_message 14
\nERROR: Insufficient data in the configuration file to properly configure 
all devices on your sound card. Make sure the following lines are defined 
in your configuration file:\n

#INSUFFICIENT_LEGACY_DATA_0
iwinit_message 15
SynthBase=
CodecBase=
DMA1=
DMA2=
IRQ1=

#INSUFFICIENT_LEGACY_DATA_1
iwinit_message 16
CDBASE=
ATAPIBase=
CDDMA=
CDIRQ=

#INSUFFICIENT_LEGACY_DATA_2
iwinit_message 17
GamePort=

#INSUFFICIENT_LEGACY_DATA_3
iwinit_message 18
AdLibBase=
SBIRQ=

#INSUFFICIENT_LEGACY_DATA_4
iwinit_message 19
MpuBase=
MpuIrq=

#IW_CARD_OFF
iwinit_message 20
InterWave card #%d turned off.
