*********************************************************************** 
 
			IMPORTANT INFORMATION 
				for 
	    Windows 95 mach64 enhanced display driver 
*********************************************************************** 
Windows 95 mach64 enhanced display driver               August  2, 1996 
*********************************************************************** 
 
READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT ! 
 
**************************** 
 
Contents 
 
1.0     Introduction 
2.0     Adapter Installation 
3.0     Installation Notes for Windows 95 mach64 enhanced display driver 
4.0     Windows 95 mach64 enhanced display driver problems 
5.0     Windows 95 property page problems 
 
 
**************************** 
 
1.0     Introduction 
 
This file contains last-minute updates that are not found in the User's 
Guide or in any addendum accompanying the display adapter.  Please read 
this file before proceeding with the installation. 
 
**************************** 
 
2.0     Adapter Installation 
 
Refer to the User's Guide for information on adapter installation. 
 
 
**************************** 
 
3.0     Installation Notes for Windows 95 mach64 enhanced display driver 
 
The Windows 95 mach64 enhanced display driver is a Windows 95 mini driver.  
It is installed and configured using the standard Windows 95 configuration 
utilities. 
									  
Note: Windows 95 will require a re-start to implement certain display 
      settings 
 
1) Start Windows 95. 
 
2) Insert the disk labelled Windows 95 into a floppy drive.
 
3) Click on the Start button. Click on the Run menu item. 
   Type A:\WIN95\SETUP.EXE in the text entry area. Press OK.

4) Follow the instructions displayed in the help.

 
**************************** 
 
4.0     Windows 95 mach64 enhanced display driver problems 
  
- The Windows 95 mach64 enhanced display driver is capable of using monitor 
   timing data contained within Windows 95. This data is selected by  
   configuring a monitor type at Windows 95 installation time or via the  
   "Settings" page of the display properties sheet. If you change the  
   selected monitor type via the "Settings" page of the display properties  
   sheet the new timing data may not take effect until after restarting  
   Windows 95. A solution to this problem is to always restart Windows 95  
   after changing the monitor type. 
 
 - The Windows 95 mach64 enhanced display driver is capable of using monitor 
   timing data contained within Windows 95. This data is selected by  
   configuring a monitor type at Windows 95 installation time or via the  
   "Settings" page of the display properties sheet. The Windows 95 mach64  
   enhanced display driver may incorrectly interpret Windows 95 monitor  
   timing data for some older monitors which require interlaced modes.  
   This may cause some options to be disabled. A solution to this problem  
   is to select one of the "(Standard monitor types)" available via the  
   settings page of the display properties sheet. 
 
 - In Windows 95, display drivers can be installed via the "Add New 
   Hardware" wizard ( although the procedure detailed in section 3.0 is 
   recommended ). When the Windows 95 mach64 enhanced display driver is 
   installed via the "Add New Hardware" wizard the "Settings" page does 
   not get installed into the mach64 display adapter property sheet.

 - In Windows 95, Rapid Resuming with the Virtual Desktop on will cause
   loss of the Virtual Desktop.  This is because Windows 95 reinitializes
   the video mode on an APM resume.  No data loss occurs.  The desktop size
   is reduced to the screen size.  Windows 95 also reinitializes the video
   mode when windows is restarted on systems with Rapid Resume.  Again, no 
   data loss occurs and the desktop size is reduced to the screen size.
   

**************************** 
 
5.0     Windows 95 property page problems 
  
- While adjusting monitor settings in the Adjustment page of the Display
  Properties sheet, your monitor could become unreadable. If this occurs,
  press the ESC key to return to your previous monitor settings.
 
