*********************************************************************** 
WINDOWS 95 ATI DISPLAY DRIVER VERSION 4.03.2139            May 14, 1997

FOR USE WITH 3D RAGE I AND VT BASED ATI PRODUCTS.
*********************************************************************** 
 
PLEASE READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT! 

***********************************************************************

Contents 

1.0  	Introduction
2.0	Installation Notes
3.0	Windows 95 Driver Features
4.0	Identifying Your ATI Product
5.0	Generating a Problem Report
6.0     ATI Contact Information

*****************************

1.0     Introduction

This display driver is certified for use with the following ATI products;

     3D XPRESSION
     VIDEO XPRESSION+ and VIDEO XPRESSION
     VIDEO CHARGER
     All other 3D RAGE I and VT based ATI products.

NOTE: We do not recommend installing this driver for use with mach64 GX or
CT product families as it may not function correctly. 

If your ATI product came pre-installed in a complete system, you may
already have a special driver version installed (eg. IBM, AST, Gateway,
NEC, Sony).  ATI graphic processors are implemented on many 3rd party
products.  You should contact your system integrator for drivers
certified for use with your system, especially if the ATI chip is
incorporated on the mainboard or motherboard.

If you are unsure of which mach64 Product you own please see the section
Identifying Your ATI Product.
  
DO NOT USE WINDOWS 95 DRIVERS with Windows 3.X or Windows NT.

*****************************

2.0    Installation Notes

The Windows 95 ATI display driver is a Windows 95 mini driver. It is 
installed and configured using the standard Windows 95 configuration 
utilities.

To uncompress W95-2139.EXE (if you have already done so please skip
steps 1 through 4) and install this driver using the following procedure.

1.  Start Windows 95.

2.  a) Select Run from the Start icon 
    OR 
    b) Use Windows Explorer to select W95-2139.EXE and skip Step #3.

3.  When asked for the file to run, enter W95-2139.EXE from the 
    directory it was downloaded into. 

4.  Follow the instructions displayed to uncompress the installation
    files into C:\ATI\SUPPORT\WIN95.

5.  The ATI DeskTop Help setup utility will be run from
    C:\ATI\SUPPORT\WIN95.

6.  Follow the instructions displayed in the help.  

7.  Restart the computer to run Windows 95 using this new driver.
 
After successfully installing the driver, you can delete the contents of
the directory C:\ATI\SUPPORT\WIN95 using the Delete ATI Temporary Files
icon.

We recommend that you keep a copy of the W95-2139.EXE, in case you need
to install the driver again.     

PLEASE NOTE: If you have not already configured your monitor type do so
now. In the PROPERTIES - SETTINGS PAGE - CHANGE DISPLAY TYPE - Monitor 
Type area, click the Change button and select the appropriate monitor.  
Click OK to apply your changes.  Click Close to return to the Settings 
page. Click "Close" or "Apply" to initiate your changes.  
 
*****************************

3.0	Windows 95 Driver Features
 
The Windows 95 display driver supports the following additional features: 

Additional Features as compared to the mach64 driver bundled with the
Windows 95 CD-ROM;

 - DirectX 3 support which includes DirectDraw and Direct 3D.

 - MPEG playback support and ATI MPEG Video Player to view MPEG-1 videos
   at 1x, 2x and full-screen on the desktop PC.

 - A Settings Page that allows for customization of desktop settings 
   such as virtual desktop size, display resolution and color depth, 
   ability to user-customize pre-set display preferences.

 - A Panning Page that allows the user to set up hotkeys to control panning
   of the desktop within a virtual desktop.

 - A Screen Adjust Page for adjusting the size and position of screen
   images along with manipulation of the display's refresh rate.

 - A Color Correction Page to allow the user to correct for color tone 
   differences between real color values and the way the monitor displays 
   them.  Control includes color spline, gamma correction and the ability 
   for user-customized preset preferences.
                             
 - Setup Wizards, on-line documentation and context-sensitive help using 
   the Windows 95 Help Wizards.

 - Monitor Adjustment: Position and size adjustment of the Windows 95
   desktop on the display monitor, refresh rate selection, ability to
   use timing information specific to the monitor selected by the user 
   (provides greater enhancement and clearer viewing) and the ability 
   to select specific display refresh rates.

 - Low Level Hardware Configuration: Ability to select the power-up 
   video mode of the graphics adapter (the mode that the adapter will be
   set to after the computer is powered-up or reset).  Color and Monochrome 
   modes are supported.

*****************************

4.0     Identifying Your ATI Product

You will find information here which will assist you in identifying
current ATI mach64 and 3D RAGE products.

ATI mach64 and 3D RAGE products have a 'SHOW SYSTEM INFORMATION' option
in the MS DOS INSTALL program, on DISK #1 or your ATI INSTALLATION 
CD-ROM (e.g. D:\UTILITY), which will report the BIOS part number. The 
BIOS part number can also be found on a white sticker attached to the 
ROM chip on your ATI card. In most cases the first three digits of the 
BIOS part number will be 112 or 113. There is a direct relationship 
between the BIOS part number and the chip type (ASIC) used on the 
various ATI products.

If you have an ATI INSTALLATION CD-ROM version 3.0 or greater and are 
running Windows 95, you can run ATISETUP.EXE and then select TOOLS from 
the menu and then SYSTEM CHECK. This will report information about which 
ATI product you have, including the BIOS part number listed in ADAPTER 
TYPE.

The following list relates the BIOS part number to the chipset and also 
the bus type. 

	BIOS Part #	Graphics Processor	BUS 

	113-193XX-XXX	GX			ISA
	113-25XXX-XXX	GX	 		PCI
	113-26XXX-XXX	GX 			VLB
	113-27XXX-XXX	GX 			VLB
	112-28XXX-XXX	GX			ISA
	113-320XX-XXX	GX 			PCI
	113-33XXX-XXX	GX 			PCI
	113-40006-XXX 	GX 			PCI

	113-321XX-XXX	CT			PCI
	113-40007-XXX	CT			PCI

	113-34XXX-XXX	VT or 3D RAGE		PCI
	113-36XXX-XXX	VT or 3D RAGE		PCI
	113-38XXX-XXX	3D RAGE			PCI
	113-40008-XXX	VT			PCI

	113-37XXX-XXX	3D RAGE II		PCI
	113-382XX-XXX 	3D RAGE II		PCI
	113-385XX-XXX	3D RAGE II		PCI
	113-4010X-XXX	3D RAGE II		PCI

 - GX chips can be found on the following ATI products 
     GRAPHICS PRO TURBO
     GRAPHICS XPRESSION
     WINTURBO 
     WINBOOST

 - CT chips can be found on the following ATI products
     GRAPHICS XPRESSION
     WINBOOST 
     WINCHARGER

 - VT Chips can be found on the following ATI products
     VIDEO XPRESSION+ and VIDEO XPRESSION
 
 - 3D RAGE chips can be found on the following ATI Product
     3D XPRESSION

 - 3D RAGE II+ or 3D RAGE II chips can be found on the following ATI 
   products
     ALL IN WONDER
     3D PRO TURBO and 3D PRO TURBO PC2TV
     3D XPRESSION+ and 3D XPRESSION+ PC2TV
     3D CHARGER

If this information does not help you please refer to the sections 
Generating a Problem Report and Contacting ATI Technical Support for help
with identifying your ATI Product.

*****************************

5.0     Generating a Problem Report

If contacting Technical Support regarding a problem you are experiencing
please complete the Problem Report Wizard in the ATI Desktop Help Wizard.

1. Right click on the red ATI Toolbar icon.

2. Select Troubleshooting.

3. Select ATI DeskTop Help.

4. From the Troubleshooting menu select Problem Report Wizard.

5. Follow the instructions displayed in the help to complete the Problem
   Report. 

Have the Problem Report available when contacting us by phone or send the
completed report to us by fax or email.

*****************************

6.0     ATI Contact Information

Telephone numbers: 
  (905) 882-2600		Head Office, Sales and Marketing
  (905) 882-2620		Corporate Fax
  (905) 882-2626		Tech Support Voice
  (905) 882-0546		Tech Support Fax 

Email:
  76004.3656@compuserve.com	Electronic Marketing
  74740,667			Tech Support Compuserve
  support@atitech.ca		Tech Support Internet

Driver Download Sites:
  www.atitech.ca		ATI World Wide Web
  support.atitech.ca		Tech Support World Wide Web
  ftp.atitech.ca		FTP Download
  (905) 764-9404		BBS Download
  [GO] ATITECH			Compuserve Forum

*****************************
