; "MDMCHIPV.INF"
; 
; Product Name: ASUS MR Series 	
; Manufacturer:	ASUSTek COMPUTER, Inc.
; Copyright 1999  PCtel, Inc
;
[Version]
Signature="$CHICAGO$"
Class=Modem
ClassGUID={4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider=%Mfg%
;CatalogFile=mdmchipv.cat
DriverVer=07/15/1999, 1.000


[DestinationDirs]
DefaultCopy1 = 12	
DefaultCopy2 = 12	
DefaultCopy3 = 12	
DefaultDestDir = 12
DataCopy = 11
PTInf.Copy=17

[Manufacturer]
%Mfg% = Models


;
; Modem models
;
[Models]     
; You're only allowed to choose one model for one submission.     
%Modem1% = Modem1,PCI\VEN_8086&DEV_2416
%Modem1% = Modem1,PCI\VEN_8086&DEV_2426
%Modem1% = Modem1,PCI\VEN_8086&DEV_2446
%Modem1% = Modem1,PCI\VEN_8086&DEV_7196
%Modem2% = Modem2,PCI\VEN_1106&DEV_3068
%Modem3% = Modem3,PCI\VEN_1039&DEV_7013

[Modem1.NT]
AddReg=All, MfgAddReg, PCTEL_VOICE_SERWAVE
CopyFiles = DefaultCopy1, DataCopy

[Modem2.NT]
AddReg=All, MfgAddReg, PCTEL_VOICE_SERWAVE
CopyFiles = DefaultCopy2, DataCopy

[Modem3.NT]
AddReg=All, MfgAddReg, PCTEL_VOICE_SERWAVE
CopyFiles = DefaultCopy3, DataCopy

;
; User visible strings
;
[Strings]
Mfg = "ASUSTek COMPUTER, Inc"
; Model strings
;
Modem1="ASUS MR Series"
Modem2="ASUS MR Series"
Modem3="ASUS MR Series"
ID1="Disk 1"

;
[DefaultCopy1]
ptserial.sys,ptserli.sy_,,6
vpctcom.sys,vpctcom.sy_,,6
vmodem.sys,vmodem.sy_,,6
vvoice.sys,vvoice.sy_,,6

[DefaultCopy2]
ptserial.sys,ptserlv.sy_,,6
vpctcom.sys,vpctcom.sy_,,6
vmodem.sys,vmodem.sy_,,6
vvoice.sys,vvoice.sy_,,6

[DefaultCopy3]
ptserial.sys,ptserls.sy_,,6
vpctcom.sys,vpctcom.sy_,,6
vmodem.sys,vmodem.sy_,,6
vvoice.sys,vvoice.sy_,,6

[DataCopy]
pthsp.dat,pthsp.da_,,6
pctspk.exe,pctspk.ex_,,6
ptuninst.exe,ptuninst.exe,,6
pctport.cp_,pctport.cp_,,6
ptsetup.dll,ptsetup.dll,,6
pctptt.exe,pctptt.ex_,,6
ptcounty.ini,ptcounty.ini,,6

[SourceDisksNames]
1=%ID1%

[SourceDisksFiles]
ptserli.sy_=1
ptserlv.sy_=1
ptserls.sy_=1
vpctcom.sy_=1
vmodem.sy_=1
vvoice.sy_=1
mdmchipv.inf=1
pthsp.da_=1
pctspk.ex_=1
pctport.cp_=1
pctptt.ex_=1
ptsetup.dll=1
ptuninst.exe=1
ptcounty.ini=1

[Modem1.NT.Services]
AddService=Ptserial,0x00000000,Ptserial_Service_Inst
AddService=Vmodem,0x00000000,Vmodem_Service_Inst
AddService=Vpctcom,0x00000000,Vpctcom_Service_Inst
AddService=Vvoice,0x00000000,Vvoice_Service_Inst
AddService=Pctspk,0x00000000,Pctspk_Service_Inst

[Modem1.NT.HW]
AddReg=LowerFilterAddReg

[Modem2.NT.Services]
AddService=Ptserial,0x00000000,Ptserial_Service_Inst
AddService=Vmodem,0x00000000,Vmodem_Service_Inst
AddService=Vpctcom,0x00000000,Vpctcom_Service_Inst
AddService=Vvoice,0x00000000,Vvoice_Service_Inst
AddService=Pctspk,0x00000000,Pctspk_Service_Inst

[Modem2.NT.HW]
AddReg=LowerFilterAddReg

[Modem3.NT.Services]
AddService=Ptserial,0x00000000,Ptserial_Service_Inst
AddService=Vmodem,0x00000000,Vmodem_Service_Inst
AddService=Vpctcom,0x00000000,Vpctcom_Service_Inst
AddService=Vvoice,0x00000000,Vvoice_Service_Inst
AddService=Pctspk,0x00000000,Pctspk_Service_Inst

[Modem3.NT.HW]
AddReg=LowerFilterAddReg
[LowerFilterAddReg]
HKR,,"LowerFilters",0x00010000,Ptserial

[Ptserial_Service_Inst]
DisplayName="W2K Pctel Serial Device Driver"
ServiceType=1
StartType=3
ErrorControl=1
ServiceBinary=%12%\ptserial.sys

[Vpctcom_Service_Inst]
DisplayName="W2k Vpctcom"
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\vpctcom.sys

[Vmodem_Service_Inst]
DisplayName="W2k Vmodem"
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\vmodem.sys

[Vvoice_Service_Inst]
DisplayName="W2k Vvoice"
ServiceType=1
StartType=0
ErrorControl=1
ServiceBinary=%12%\vvoice.sys

[Pctspk_Service_Inst]
DisplayName="W2k PCtel speaker phone"
ServiceType=16
StartType=2
ErrorControl=1
ServiceBinary=%10%\system32\pctspk.exe
;
; AddReg sections
;

; --------------------------------------------------------------
; Common Registry Sections
;
; The [All] section is installed for all modems.
;
[All]
HKLM,"system\currentcontrolset\services\ptserial",ChipSet,0x00010001,2
HKLM,"system\currentcontrolset\services\ptserial",FixMidi,0x00010001,2
HKLM,"Software\PCTEL\HSPModem\Settings",language,0x00010001,0
HKLM,"Software\Microsoft\Windows\CurrentVersion\Uninstall\Installing HSP56 MicroModem Drivers",UninstallString,,"ptuninst.exe"
HKLM,"Software\Microsoft\Windows\CurrentVersion\Uninstall\Installing HSP56 MicroModem Drivers",DisplayName,,"ASUS MR Series"
HKR,, DeviceType, 1, 02      ; Internal
HKR,, Properties, 1, 80,01,00,00, ff,00,00,00, ff,00,00,00, 00,00,00,00, 0f,00,00,00, f7,07,00,00, 00,c2,01,00, C0,DA,00,00
HKR,,PortSubClass,1,02
HKR,,ConfigDialog,,modemui.dll
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"
;
;


[MfgAddReg]
HKR,, InactivityScale, 1, 0a,00,00,00
HKR,, InactivityFormat,, "seconds"
HKR, Init,      1,, "AT<cr>"
HKR, Init,      2,, "AT&FE1&C1&D2&K3V1W3S0=0<cr>"
HKR, Monitor,   1,, "ATS0=0<cr>"
HKR, Monitor,   2,, "None"
HKR, Hangup,    1,, "ATH<cr>"
HKR, Answer,    1,, "ATA<cr>"
HKR,, Reset,, "AT&F<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, SpeakerMode_Off,, "M0"
HKR, Settings, SpeakerMode_Dial,, "M1"
HKR, Settings, SpeakerMode_On,, "M2"
HKR, Settings, SpeakerMode_Setup,, "M3"
HKR, Settings, FlowControl_Off,, "&K0"
HKR, Settings, FlowControl_Hard,, "&K3"
HKR, Settings, FlowControl_Soft,, "&K4"
HKR, Settings, ErrorControl_Off,, "\N0"
HKR, Settings, ErrorControl_Forced,, "\N2"
HKR, Settings, ErrorControl_On,, "\N3"
HKR, Settings, Compression_Off,, "%%C0"
HKR, Settings, Compression_On,, "%%C3"
HKR, Settings, Modulation_CCITT,, "B0"
HKR, Settings, Modulation_Bell,, "B1"    
HKR, Settings, Modulation_CCITT_V23,,"B2"
HKR, Settings, SpeedNegotiation_Off,, "N0S37=14"
HKR, Settings, SpeedNegotiation_On,, "N1"
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"
HKR, Settings, Blind_Off,,"X4"
HKR, Settings, Blind_On,,"X1"
HKR, Settings, CallSetupFailTimer,, "S7=<#>"
HKR, Settings, InactivityTimeout,, "S30=<#>"

;       
HKR, Responses, "0<cr>", 1, 00, 00, 00,00,00,00, 00,00,00,00 ; OK
HKR, Responses, "1<cr>", 1, 02, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "2<cr>", 1, 08, 00, 00,00,00,00, 00,00,00,00 ; RING
HKR, Responses, "3<cr>", 1, 04, 00, 00,00,00,00, 00,00,00,00 ; NO CARRIER
HKR, Responses, "4<cr>", 1, 03, 00, 00,00,00,00, 00,00,00,00 ; ERROR
HKR, Responses, "5<cr>", 1, 02, 00, b0,04,00,00, 00,00,00,00
HKR, Responses, "6<cr>", 1, 05, 00, 00,00,00,00, 00,00,00,00 ; NO DIALTONE
HKR, Responses, "7<cr>", 1, 06, 00, 00,00,00,00, 00,00,00,00 ; BUSY
HKR, Responses, "8<cr>", 1, 07, 00, 00,00,00,00, 00,00,00,00 ; NO ANSWER

; The Verbose form for response
;
HKR, Responses, "<cr>", 1, 01, 00, 00,00,00,00, 00,00,00,00               ;00
HKR, Responses, "<lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00               ;00

HKR, Responses, "<cr><lf>OK<cr><lf>", 1, 00, 00, 00,00,00,00, 00,00,00,00		;00
HKR, Responses, "<cr><lf>RING<cr><lf>", 1, 08, 00, 00,00,00,00, 00,00,00,00		;02
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>", 1, 04, 00, 00,00,00,00, 00,00,00,00	;03
HKR, Responses, "<cr><lf>ERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;04
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00	;06
HKR, Responses, "<cr><lf>BUSY<cr><lf>", 1, 06, 00, 00,00,00,00, 00,00,00,00		;07
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>", 1, 07, 00, 00,00,00,00, 00,00,00,00	;08
HKR, Responses, "<cr><lf>RING BACK<cr><lf>", 1, 01, 00, 00,00,00,00, 00,00,00,00	;25
HKR, Responses, "<cr><lf>+FCERROR<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;+F4
HKR, Responses, "<cr><lf>FAX<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;33
HKR, Responses, "<cr><lf>DATA<cr><lf>", 1, 03, 00, 00,00,00,00, 00,00,00,00		;35

HKR,Responses,"<cr><lf>CONNECT<cr><lf>", 1, 02, 00, 00,00,00,00, 00,00,00,00		;01
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 300/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,2C,01,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/75/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 75/1200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 1200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,04,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 2400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,09,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 4800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,12,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 7200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,1C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 9600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,25,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 12000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,2E,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 14400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,38,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 16800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,A0,41,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 19200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,00,4B,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 21600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,54,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 24000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,5D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 26400/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,67,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,60,6D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 28800/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,70,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 29333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,95,72,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 30666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,CA,77,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 31200/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,79,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33600/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,83,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 32000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,00,7D,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 33333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,35,82,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,D0,84,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 34666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,6A,87,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 36000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,A0,8C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 37333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,D5,91,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,70,94,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 38666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,0A,97,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 40000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,40,9C,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 41333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,75,A1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,10,A4,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 42666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,AA,A6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 44000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,E0,AB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 45333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,15,B1,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B0,B3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 46666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,4A,B6,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 48000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,80,BB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 49333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,B5,C0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,50,C3,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 50666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,EA,C5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 52000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,20,CB,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 53333/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,55,D0,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,F0,D2,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 54666/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,8A,D5,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: NONE/COMPRESSION: NONE<cr><lf>",1,02,00,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: LAPM/COMPRESSION: NONE<cr><lf>",1,02,02,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: LAPM/COMPRESSION: V.42bis<cr><lf>",1,02,03,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: ALT/COMPRESSION: NONE<cr><lf>",1,02,02,C0,DA,00,00,00,00,00,00
HKR,Responses,"<cr><lf>CONNECT 56000/PROTOCOL: ALT/COMPRESSION: CLASS 5<cr><lf>",1,02,03,C0,DA,00,00,00,00,00,00

[PCTEL_VOICE_SERWAVE]   ; PCtel serial wave settings
HKR,, VoiceProfile,                     1, 23,10,01,02
HKR,, HandsetCloseDelay,                1, 8,00,00,00
HKR, StartPlay,                         1,, "at#vtx<cr>"
HKR, StopPlay,                          1,, "None"
HKR, StopPlay,                          2,, "NoResponse"
HKR, StartRecord,                       1,, "at#vrx<cr>"
HKR, StopRecord,                        1,, "None"
HKR, StopRecord,                        2,, "NoResponse"
HKR,, TerminateRecord,,                 "<h10>E"
HKR,, TerminatePlay,,                   "<h10><h03>"
HKR,, AbortPlay,,                       "<h10><h18>"
HKR, LineSetPlayFormat,                 1,, "at#vls=0<cr>"
HKR, LineSetPlayFormat,                 2,, "at#tl=7fff<cr>"
HKR, LineSetRecordFormat,               1,, "None"
HKR, LineSetRecordFormat,               2,, "NoResponse"
HKR, HandsetSetRecordFormat,            1,, "at#vsr=8000<cr>"
HKR, HandsetSetRecordFormat,            2,, "at#vbs=4<cr>"
HKR, HandsetSetPlayFormat,              1,, "at#vsr=8000<cr>"
HKR, HandsetSetPlayFormat,              2,, "at#vbs=4<cr>"
HKR, OpenHandset,                       1,, "at#cls=8#ima=1<cr>"
HKR, OpenHandset,                       2,, "at#vls=1<cr>"
HKR, CloseHandset,                      1,, "at#vls=0<cr>"
HKR, CloseHandset,                      2,, "at#ima=0#cls=0<cr>"
HKR, VoiceToDataAnswer,                 1,, "at#ima=0#cls=0<cr>"
HKR, VoiceToDataAnswer,                 2,, "ata<cr>"
HKR, VoiceAnswer,                       1,, "at#cls=8#ima=1<cr>"
HKR, VoiceAnswer,                       2,, "at#vls=0<cr>"
HKR, VoiceAnswer,                       3,, "at#vbt=1<cr>"
HKR, VoiceAnswer,                       4,, "ats30=60<cr>"
HKR, VoiceAnswer,                       5,, "ata<cr>"
HKR, VoiceDialNumberSetup,              1,, "at#cls=8#ima=1<cr>"
HKR, VoiceDialNumberSetup,              2,, "at#vls=0<cr>"
HKR, VoiceDialNumberSetup,              3,, "at#vrn=0<cr>"
HKR, VoiceDialNumberSetup,              4,, "at#vbt=1<cr>"
HKR, VoiceDialNumberSetup,              5,, "ats30=60<cr>"

HKR, WaveDriver, XformModule,  , "umdmxfrm.dll"
HKR, WaveDriver, XformID,     1, 04, 00
HKR, WaveDriver, BaudRate,    1, 00, c2, 01, 00
HKR, WaveDriver, WaveDevices, 1, 02, 00
HKR, WaveDriver, WaveHardwareID, , "FullDuplex"

HKR,, VoiceManufacturerID,  1, 01,00
HKR,, VoiceProductIDWaveIn, 1, 80,00
HKR,, VoiceProductIDWaveOut,1, 81,00
HKR,, VoiceProductIDHandsetWaveIn,1, 82,00
HKR,, VoiceProductIDHandsetWaveOut,1, 83,00
HKR,, VoiceMixerMid,          1,02,00
HKR,, VoiceMixerPid,          1,99,01
HKR,, VoiceMixerLineID,       1,00,00,05,00

HKR,, CallerIDPrivate,,         "P"
HKR,, CallerIDOutside,,         "O"
HKR, EnableCallerID, 1,, "at#cid=1<cr>"
HKR, DisableCallerID, 1,, "at#cid=0<cr>"
HKR,, VariableTerminator,,<cr><lf>
HKR, GenerateDigit,           1,, "at#vts=<Digit><cr>"

HKR, Responses, "VCON", 1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "DATE = ", 1, 93, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "TIME = ", 1, 94, 00, 00,00,00,00, 00,00,00,00            
HKR, Responses, "NMBR = ", 1, 95, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "NAME = ", 1, 96, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "MESG = ", 1, 97, 00, 00,00,00,00, 00,00,00,00

