United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic discharge
Service considerations
Preparation for disassembly
Serial number
Hood
Fax-modem
System board bracket
Serial port assembly
Mass storage devices
System board components
Power supply
Front bezel
Instant On button board
Creativity Action Center
| REMOVAL & REPLACEMENT Power Supply
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
4 | Remove the system board bracket
5 | Disconnect the power cables to these mass storage devices: 3.5" hard drive or 5.25" hard drive CD or DVD drive Zip drive diskette drive
6 | Remove the four screws that secure the power supply to the rear of the chassis
7 | Slide the power supply back and remove from the chassis.
To replace the power supply, reverse this procedure.

privacy and legal statement