United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic discharge
Service considerations
Preparation for disassembly
Serial number
Hood
Fax-modem
System board bracket
Serial port assembly
Mass storage devices
System board components
Power supply
Front bezel
Instant On button board
Creativity Action Center
| # REMOVAL & REPLACEMENT ## Preparation for Disassembly To prepare the computer for removal and replacement procedures, complete the following steps:
1 | Remove any diskette, compact disc, or tape from the computer.
2 | Turn off the computer and any peripheral devices that are connected to the computer.
> | CAUTION: The computer power switch should be turned off before you disconnect any cables.
3 | Disconnect the power cord from the electrical outlet, and then from the computer.
4 | Disconnect all peripheral device cables from the computer.
> IMPORTANT: | During disassembly, label each cable as you remove it. Be sure to note its position and routing.
privacy and legal statement