United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic discharge
Service considerations
Preparation for disassembly
Serial number
Hood
Fax-modem
System board bracket
Serial port assembly
Mass storage devices
System board components
Power supply
Front bezel
Instant On button board
Creativity Action Center
| REMOVAL & REPLACEMENT Serial Port Cable Assembly
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
| CAUTION: Remove the fax/modem before removing the system board bracket, or the system board may be damaged.
4 | Open the system board bracket
5 | Remove the two screwlocks that secure the serial port to the chassis and pull the serial port cable assembly out of the chassis
To replace the serial port, reverse this procedure.
privacy and legal statement