United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
Processor & goalposts
Memory module
Video memory
Battery
System board
Heat sink clip
I-O panel
Cache
System board components index page
l
| REMOVAL & REPLACEMENT System Board Components Removing the Cache (4910 Model only)
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
4 | Open the system board bracket
5 | Gently pull out the cache from the socket on the system board
To replace the cache, reverse this procedure.
privacy and legal statement