United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
3.5" Diskette Drive
3.5" Hard drive
5.25" Hard drive
CD or DVD drive
Zip drive
Mass storage devices index page
l
| REMOVAL & REPLACEMENT Mass Storage Devices 5.25" Hard Drive
| There are seven steps in this sequence.
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
| CAUTION: The fax/modem must be removed before the system board bracket, or the system board may be damaged.
4 | Open the system board bracket
5 | Disconnect the signal and power cables from the hard drive.
NEXT STEP
privacy and legal statement