United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
| REMOVAL & REPLACEMENT Removing the System Board Bracket, continued
10 | Slide the system board bracket back at an angle, lining up the pins in the top and bottom with the hinge opening, then pull the system board bracket out of the chassis.
END OF SEQUENCE To replace the system board bracket, reverse this procedure.
| CAUTION: When replacing the system board bracket, ensure the fingers of the I/O bracket are properly aligned to prevent bending the fingers. Bending the bracket fingers may damage the system board.
Return to section index
privacy and legal statement