United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
DISASSEMBLY SEQUENCE
Electrostatic discharge
Service considerations
Preparation for disassembly
Serial number
Hood
Fax-modem
System board bracket
Serial port assembly
Mass storage devices
System board
Power supply
Front bezel
Instant On button board
Creativity Action Center
| REMOVAL & REPLACEMENT System Board Bracket
| There are ten steps in this procedure.
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
CAUTION: The fax/modem must be removed before the system board bracket, or damage may occur to the system board.
4 | Remove the screws from the top and the side of the system board bracket and chassis.
NEXT STEP

privacy and legal statement