United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
Processor & goalposts
Memory module
Video memory
Battery
System board
Heat sink clip
I-O panel
Cache
System board components index page
l
| REMOVAL & REPLACEMENT System Board Components Removing the Heat Sink Clip (on selected models)
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax-modem
4 | Remove the system board bracket
5 | Remove the processor
6 | Remove the system board and separate it from the bracket
7 | Locate the two inserts under the system board that secure the heat sink clip and unplug from the system board
8 | Remove the heat sink clip from the system board
To replace the heat sink clip, reverse this procedure.
privacy and legal statement