United States
Maintenance and Service Guide Compaq Presario 4900, 5000, & 5100 Series Computers
Home | Product Description | Troubleshooting | Illustrated Parts Catalog
Removal & Replacement | Jumper & Switch Information | Specifications
3.5" Diskette drive
3.5" Hard drive
5.25" Hard drive
CD or DVD drive
Zip drive
Mass storage devices index page
l
| REMOVAL & REPLACEMENT Mass Storage Devices Zip Drive
| There are eight steps in this sequence.
1 | Perform preparation procedures
2 | Remove the hood
3 | Remove the fax/modem
| CAUTION: If the fax/modem is not removed before the system board bracket, damage may occur to the system board.
4 | Open the system board bracket
5 | Disconnect the signal and power cables from the Zip drive.
NEXT STEP

privacy and legal statement