United States
Maintenance and Service Guide Compaq Presario 7300 Series Computers
| Product Description | Troubleshooting | Illustrated Parts Catalog
Home | Removal & Replacement | Jumper & Switch Information | Specifications
System
Power supply
Diskette drive
Hard drives
CD drive
Mouse
Fax/modem
| SPECIFICATIONS CD Drive Information for the 32x CD drive immediately follows.
32× CD Drive
Dimensions | U. S. | Metric
Width Height Depth | in in in | cm cm cm
Weight | lb | kg
Modes Supported |
CD-ROM CD-DA CD-XA Photo CD Video-CDI CD-Plus/CD-Extra/CD Enhanced CD-RW | Mode 1 and Mode 2 Audio Mode 2, Form 1 and 2 Multiple Session Multiple Session Multiple Session Multiple Session
Block Size |
CD-ROM Mode 1 and Mode 2 Form 1 (XA) CD-ROM Mode 2 CD-DA CD-XA | 2048 bytes 2336 bytes 2324 bytes 2324 bytes
Center Hole | 1.5 mm diameter
Diameter | 120 mm / 80mm
Thickness | 1.2 mm
Track Pitch | 1.6 µm
Access Time |
Random Full Stroke | < 95 ms < 190 ms
Audio Output Level |
Line Out Headphone | 0.7 Vrms + 20% 0.6 Vrms + 20%
Cache Buffer | 256 KB
Data Transfer Rate |  |
Sustained Burst | Mode 1 4800 KB/sec KB/sec (32×) MB/sec | Mode 2 5475 KB/sec KB/sec (32×) MB/sec
Startup Time | < 5 sec
Stop Time | < 5 sec
privacy and legal statement