		GDS546X Windows 3.1x Driver 1.52 Release
		--------------------------------------------------

Changes to 1.52 since 1.47a
===========================

Files modified:
546X.DRV, DVDD546X.386, INSTALL.INF, JVDD546X.386, VDD546X.386, WINMODE.INI

Problems solved/New features:

-Fixed corruption of gray text in Print Manager from Program Manager 
  occurring in 64K. PDR#10276.

-Fixed filled black characters in MS-Excel (Japanese only). PDR#10281.

-Fixed Lotus Organizers text tabs displaying black and white colors 
  occurring in 64K. PDR#10282.

-Reduced display driver usuage in conventional memory. PDR#10287.

-Fixed corrupted line appearing in Icon bar under CAD/DRAW in Wintech1.2. 
  PDR#10277.

-Fixed corrupted lines in the demo window in AfterDark when selecting 
  Hard Rain. PDR#10280.

-Resolved proper display in AfterDark when selecting Ship Panels and Display. 
  (Japanese only). PDR#10278.

-Resolved proper display of clouds in AfterDark Space/Demo selection.
  (Japanese only). PDR#10279.

-Corrected display of background color and text in the Calendar tab 
  and ToDo tab when launching Windows3.1 then Lotus Organizer. PDR#10283

-Fixed system locks up when loading File Manager or changing resolution via Winmode.exe.


How to install 546X Windows 3.1 Driver
======================================

Prior to installing these drivers, Make sure that Windows is using
the VGA driver that was included with Windows. If Windows is using any other 
driver, reconfigure Windows using Setup from DOS or from within Windows.

1. Insert the 546X Windows 3.1x Driver Installation diskette into A: or B:.
2. Run INSTALL.EXE on the diskette from Windows File Manager.
3. Follow instructions on screen to complete the installation process.
4. A WinMode program will pop up to ask user to select options.  Select
   any desired choice to fit your preference.


Known Problems
==============

- Character corruption remaining on screen in ExpertCAD after screen drawing 
   is erased. Relates to Bitmap capture 10284_3.bmp and 10284_5.bmp. PDR#10284.

- The third and fourth screen image doesn't display properly in Corel 
   when selecting RunScreenShow. PDR#10285.

- Improper printing occurs in EX-PR-H1.EJS file in MS-Excel.


Windows 3.1 driver limitation
=============================

-Windows 3.1x will prompt user to restart when changing resolution, colors, 
 and monitor refresh rate via Winmode.


Diskette Contents
=================

546X Windows 3.1x Installation Disk

Files w/ extentions .xx_ are compressed.

README   1ST                    09-12-97
VGACOLOR 2G_                    03-10-92
JVDD546X 386    R119.24	        09-10-97
DVDD546X 38_    R119.24	        09-10-97
VDD546X  38_    R119.24	        09-10-97
AVGA     3G_                    03-10-92
TIMINGS  DA_                    09-01-95
CTL3D    DLL                    05-05-95
INSTLANG DLL                    05-10-95
LAGUNA   DLL                    07-31-96
MSVIDEO  DL_                    03-17-95
UDH      DL_                    09-28-94
WINMODEL DL_    V2.2            09-10-96
WM5462   DL_    V2.20.546X      07-19-97
WM5462L  DL_    V2.20.546X      07-19-97
546X     DR_    R119.24	        09-18-97
DCI546X  DR_                    07-16-97
ICCVID   DR_                    05-09-95
INSTALL  EXE                    05-21-95
WINMODE  EX_    V2.20.546X      07-19-97
WINMODE  HL_                    04-26-95
INSTALL  INF                    09-19-97
WINMODE  INI                    09-12-97
OEM546X  IN_                    09-12-97

