 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 1
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
ADAPTEC           ACB-2010       ISA-ST412(MFM)   2HD      PC,XT                             XT                             
ADAPTEC           ACB-2070       ISA-ST412(RLL)   2HD      PC,XT                             XT                             
ADAPTEC           ACB-2071       ISA-ST412(RLL)   1HD      XT                                XT                             
ADAPTEC           ACB-2072       ISA-ST412(RLL)   2HD      PC,XT     2:1  16 2048  B    1/2  XT                             
ADAPTEC           ACB-2310       ISA-ST412(MFM)   2HD      PC,XT,AT  1:1                     XT                             
ADAPTEC           ACB-2312       ISA-ST412(MFM)   2HD 2FD  PC,XT,AT                          XT                             
ADAPTEC           ACB-2320       ISA-ESDI         2HD      AT        1:1  16 4096  B    3/4  XT                             
ADAPTEC           ACB-2322       ISA-ESDI         2HD 2FD  AT        1:1  16 4096  B    FULL XT                             
ADAPTEC           ACB-2370       ISA-ST412(RLL)   2HD      AT        1:1  16 4096  B    3/4  XT                             
ADAPTEC           ACB-2372       ISA-ST412(RLL)   2HD 2FD  AT        1:1  16 4096  B    FULL XT                             
ADAPTEC           ACB-2610       MCA-ST412(MFM)   2HD      MCA       1:1  16 4096       FULL MC   CACHE, TRACK BUFFER       
ADAPTEC           ACB-2670       MCA-ST412(RLL)   2HD      MCA       1:1           *    FULL MC   CACHE, BUFFER, *OPTION    
ADAPTEC           ACB-26M20      MCA-ESDI         2HD      MCA       1:1  16 4096       FULL MC   CACHE, BUFFER             
ADAPTEC           ACB-3530       SCSI-QIC36                NONE                                   (TAPE) DOES NOT PLUG-IN   
ADAPTEC           ACB-3540       SCSI-QIC120               NONE                                   (TAPE) DOES NOT PLUG-IN   
ADAPTEC           ACB-4000A      SCSI-ST412(MFM)  2HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-4070       SCSI-ST412(RLL)  2HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-4520       SCSI-ESDI        2HD      NONE      1:1                          DOES NOT PLUG-IN          
ADAPTEC           ACB-4525Z      SCSI-ESDI        2HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-5500       SCSI-ST412(MFM)  2HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-5580A      SCSI-SMD         4HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-5580D      SCSI(DIF.)-SMD   4HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-5585A      SCSI-ESMD        4HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           ACB-5585D      SCSI(DIF.)-ESMD  4HD      NONE      1:1  16                      DOES NOT PLUG-IN          
ADAPTEC           AHA-1020       ISA-SCSI         7HD      PC,XT,AT                B C  1/2  XT   HOST ADAPTER              
ADAPTEC           AHA-1540A      ISA-SCSI         7HD      AT                      B    FULL XT   HOST ADAPTER              
ADAPTEC           AHA-1542A      ISA-SCSI         7HD 2FD  AT                      B    FULL XT   HOST ADAPTER              
ADAPTEC           AHA-1640       MCA-SCSI         7HD      MCA                          FULL MC   HOST ADAPTER, BUS MASTER  
AMS               1100S          ISA-ST412(MFM)   2HD 2FD  AT                                                               
AMS               1100SM         ISA-ST412(MFM)   2HD 2FD  AT        1:1                                                    
AMS               1100SM4        ISA-ST412(MFM)   2HD 4FD  AT        1:1                                                    
AMS               1100SR4        ISA-ST412(RLL)   2HD 4FD  AT        1:1                          SHORT CARD                
COGENT DATA TECH. DISKMASTER     ISA-ST412/ESDI   4HD      AT        1:1                          DISK MIRRORING            
COMMAX TECH.      EXCELL-HDC6V   ISA-ST412(MFM)   2HD 2FD  AT        1:1                3/4  XT                             
COMPUADD          HARDCACHE ESDI ISA-ESDI         2HD 2FD  AT        1:1           B    FULL XT   .25-4MB CACHE             
D.P.T.            PM3011/50      ISA-ST412(MFM)   2HD      AT        1:1                FULL                                
D.P.T.            PM3011/60      ISA-ST412(RLL)   2HD      AT        1:1                FULL                                
D.P.T.            PM3011/70      ISA-ESDI         2HD      AT        1:1                FULL                                
D.P.T.            PX3011/05      ISA-FLOPPY           2FD                                         PM3011 ADD-ON BOARD       
D.P.T.            PX3011/059     ISA-FLOPPY/SCSI  7HD 2FD                                         PM3011 ADD-ON BOARD       
D.P.T.            PX3011/09      ISA-SCSI         7HD                                             PM3011 ADD-ON BOARD       
 
 
 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 2
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
DATA TECHNOLOGY   DTC-3150       ISA-SCSI         7HD      XT,AT                   B C  1/2  XT   HOST ADAPTER              
DATA TECHNOLOGY   DTC-3180       ISA-SCSI         7HD      AT                      B C  1/2  XT   HOST ADAPTER              
DATA TECHNOLOGY   DTC-3250       ISA-SCSI         7HD 3FD  XT,AT                   B C  1/2  XT   HOST ADAPTER              
DATA TECHNOLOGY   DTC-3280       ISA-SCSI         7HD 4FD  AT                      B C  1/2  XT   HOST ADAPTER              
DATA TECHNOLOGY   DTC-5110       ISA-FLOPPY           3FD  XT,AT                        1/2  XT   FLOPPY ONLY               
DATA TECHNOLOGY   DTC-5150X      ISA-ST412(MFM)   2HD      XT        2:1  16 2048  B    1/2  XT                             
DATA TECHNOLOGY   DTC-5150XL     ISA-ST412(MFM)   2HD      XT        2:1  16 2048  B C  1/2  XT                             
DATA TECHNOLOGY   DTC-5160X      ISA-ST412(RLL)   2HD      XT        2:1  16 2048  B    1/2  XT                             
DATA TECHNOLOGY   DTC-5160XL     ISA-ST412(RLL)   2HD      XT,AT     2:1  16 2048  B C  1/2  XT                             
DATA TECHNOLOGY   DTC-5180i      ISA-ST412(MFM)   2HD      AT             16 2048    C  1/2  XT   PWR. CONN. ON BOARD       
DATA TECHNOLOGY   DTC-5187i      ISA-ST412(RLL)   2HD      AT             16 2048  B C  1/2  XT   PWR. CONN. ON BOARD       
DATA TECHNOLOGY   DTC-5280i      ISA-ST412(MFM)   2HD 2FD  AT             16 2048       FULL XT                             
DATA TECHNOLOGY   DTC-5287i      ISA-ST412(RLL)   2HD 2FD  AT             16 2048  B    FULL XT                             
DATA TECHNOLOGY   DTC-6180       ISA-ESDI         2HD      AT        1:1  16 4096  B    FULL XT                             
DATA TECHNOLOGY   DTC-6180-15C   ISA-ESDI         2HD      AT        1:1  16 *     B    FULL      .5-4MB CACHE, *>1024      
DATA TECHNOLOGY   DTC-6180-15T   ISA-ESDI         2HD      AT        1:1  16 *     B    3/4       TRACK BUFFER, *>1024      
DATA TECHNOLOGY   DTC-6280       ISA-ESDI         2HD 2FD  AT        1:1  16 4096  B    FULL XT                             
DATA TECHNOLOGY   DTC-6280-15C   ISA-ESDI         2HD 4FD  AT        1:1  16 *     B    FULL      .5-4MB CACHE, *>1024      
DATA TECHNOLOGY   DTC-6280-15T   ISA-ESDI         2HD 4FD  AT        1:1  16 *     B    3/4       TRACK BUFFER, *>1024      
DATA TECHNOLOGY   DTC-6280SE-15C EISA-ESDI        4DH      EISA      1:1                          .5-4MB CACHE, BUS MASTER  
DATA TECHNOLOGY   DTC-7180       ISA-ST412(MFM)   2HD      AT        1:1  16 2048    C  1/2  XT   PWR. CONN. ON BOARD       
DATA TECHNOLOGY   DTC-7187       ISA-ST412(RLL)   2HD      AT        1:1  16 2048  B C  1/2  XT   PWR. CONN. ON BOARD       
DATA TECHNOLOGY   DTC-7280       ISA-ST412(MFM)   2HD 2FD  AT        1:1  16 2048       FULL XT                             
DATA TECHNOLOGY   DTC-7287       ISA-ST412(RLL)   2HD 2FD  AT        1:1  16 2048  B C  FULL XT                             
EMULEX CORP.      IB-01          ISA-SCSI         7HD      PC,XT                                  HOST ADAPTER              
EMULEX CORP.      IB-02          ISA-SCSI         7HD      AT                                     HOST ADAPTER              
EVEREX CORP.      EV-332         ISA-ST412(MFM)   2HD 2FD  AT                                                               
EVEREX CORP.      EV-346         ISA-ST412(MFM)   2HD 2FD  AT        1:1                                                    
FARADAY           FE5140         ISA-FLOPPY           4FD  PC,XT                        1/2  XT   FLOPPY ONLY               
FUTURE DOMAIN     MCS-350        MCA-SCSI         7HD      MCA                          FULL MC   HOST ADAPTER              
FUTURE DOMAIN     TMC-830        ISA-SCSI         7HD      PC,XT,AT                     1/2  XT   HOST ADAPTER              
FUTURE DOMAIN     TMC-841        ISA-SCSI         7HD      PC,XT,AT                     1/2  XT   HOST ADAPTER              
FUTURE DOMAIN     TMC-841RL      ISA-SCSI         7HD      PC,XT,AT                     1/2  XT   ROMLESS HOST ADAPTER      
FUTURE DOMAIN     TMC-870        ISA-SCSI         7HD 4FD  PC,XT,AT                     3/4  XT   HOST ADAPTER              
FUTURE DOMAIN     TMC-881        ISA-SCSI         7HD 2FD  AT                           3/4  XT   HOST ADAPTER              
INTERPHASE CORP.  4810 BARRACUDA EISA-2/SCSI      12H      EISA      1:1                          2 SCSI CHANS, 128K BUFF.  
KIMPSION          WA3-16         ISA-ST412(MFM)   2HD 2FD  AT        1:1  16 2048       3/4  XT                             
KIMPSION          WA6-V          ISA-ST412(MFM)   2HD 2FD  AT        2:1  16 2048       3/4  XT                             
KONAN CORP.       TNT-1000       ISA-ST412(MFM)   2HD      AT        1:1                     XT                             
KONAN CORP.       TNT-1050       ISA-ST412(MFM)   2HD 2FD  AT        1:1                     XT                             
LOMAS DATA PROD.  LDP CACHE II   ISA-SCSI         7HD 2FD  AT                                     HOST ADAPTER              
 
 
 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 3
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
LONGSHINE         6210D          ISA-ST412(MFM)   2HD      XT                                XT   XT ONLY                   
LONGSHINE         6220           ISA-ST412(MFM)   2HD 2FD  XT                                XT   XT ONLY                   
LONGSHINE         6220ASIC       ISA-ST412(MFM)   2HD      AT        2:1                                                    
LONGSHINE         6617           ISA-ST412(RLL)   2HD      AT        2:1                                                    
LONGSHINE         6620ASIC       ISA-ST412(MFM)   2HD 2FD  AT        2:1                                                    
LONGSHINE         6622           ISA-ST412(MFM)   2HD 2FD  AT        1:1                                                    
LONGSHINE         6627           ISA-ST412(RLL)   2HD 2FD  AT        2:1                                                    
LONGSHINE         FDC+           ISA-FLOPPY           2FD  PC,XT,AT                               FLOPPY ONLY               
MANZANTA MICROSYS 3RD INTN. MUX  ISA-FLOPPY           3FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
MANZANTA MICROSYS HI-DENS.CONTR. ISA-FLOPPY           4FD  PC,XT                        1/2  XT   FLOPPY ONLY               
MANZANTA MICROSYS MUX ADAPT.CARD ISA-FLOPPY           2FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
MICRO SOLUTIONS   COMPATICARD    ISA-FLOPPY           4FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
MICRO SOLUTIONS   COMPATICARD II ISA-FLOPPY           2FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
MICRO SOLUTIONS   COMPATICARD IV ISA-FLOPPY           4FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
MYLEX CORP.       DC-376         32BIT-SCSI       7HD      32BIT AT  1:1                FULL XT   32BIT, 4MEG CACHE         
MYLEX CORP.       DCE-376        EISA-SCSI        7HD 2FD  EISA      1:1                FULL XT   8MB CACHE (MAX)           
NCL AMERICA       NCL-3016       SCSI-ST412(MFM)  2HD      NONE           16 2048    C            DOES NOT PLUG-IN          
NCL AMERICA       NCL-3026       SCSI-ST412(RLL)  2HD      NONE           16 2048    C            DOES NOT PLUG-IN          
NCL AMERICA       NCL-500        ISA-SCSI         7HD      XT,AT                        1/2  XT   HOST ADAPTER              
NCL AMERICA       NCL-5034       ISA-FLOPPY           2FD  PC,XT,AT                     1/2  XT   FLOPPY ONLY               
NCL AMERICA       NCL-5235       ISA-ST412(RLL)   2HD 2FD  AT             16 2048       1/2  XT                             
NCL AMERICA       NCL-5236       ISA-ST412(RLL)   2HD      AT             16 2048       1/2  XT                             
NCL AMERICA       NCL-5255       ISA-ST412(RLL)   2HD 2FD  AT        1:1  16 2048       1/2  XT                             
NCL AMERICA       NCL-5256       ISA-ST412(RLL)   2HD      AT        1:1  16 2048       1/2  XT                             
NCL AMERICA       NCL-5335       ISA-ESDI         2HD 2FD  AT        1:1  16 2048       3/4  XT                             
NCL AMERICA       NCL-5336       ISA-ESDI         2HD      AT        1:1  16 2048       1/2  XT                             
NCL AMERICA       NCL-5355       ISA-ESDI         2HD 2FD  AT        1:1  16 2048       3/4  XT                             
NCL AMERICA       NCL-5356       ISA-ESDI         2HD      AT        1:1  16 2048       1/2  XT                             
NCL AMERICA       NCL-5425       ISA-ST412(MFM)   2HD 2FD  AT             16 2048       1/2  XT                             
NCL AMERICA       NCL-5426       ISA-ST412(MFM)   2HD      AT             16 2048       1/2  XT                             
NCL AMERICA       NCL-5455       ISA-ST412(MFM)   2HD 2FD  AT             16 2048       1/2  XT                             
NCL AMERICA       NCL-5456       ISA-ST412(MFM)   2HD      AT        1:1  16 2048       1/2  XT                             
NCL AMERICA       NCL-5525       ISA-ST412(MFM)   2HD 2FD  AT             16 2048       1/2  XT                             
PERCEPTIVE SOLS.  816SPU MAIN BD ISA-PROPRIETARY           AT                           FULL      MAIN BOARD & STORAGE CPU  
PERCEPTIVE SOLS.  DIAL RLL ADAPT PRO.-ST412(RLL)  2HD      AT        1:1  16 2048  B C            1600 ADD-ON BOARD (4 MAX) 
PERCEPTIVE SOLS.  DUAL ESDI ADPT PRO.-ESDI        2HD      AT        1:1           B C            1600 ADD-ON BOARD (4 MAX) 
PERCEPTIVE SOLS.  DUAL MFM ADAPT PRO.-ST412(MFM)  2HD      AT        1:1  16 2048  B C            1600 ADD-ON BOARD (4 MAX) 
PERCEPTIVE SOLS.  DUAL MFM ADAPT PRO.-ST412(MFM)  2HD      AT        1:1  16 2048  B C            816SPU ADD-ON BOARD       
PERCEPTIVE SOLS.  DUAL RLL ADAPT PRO.-ST412(RLL)  2HD      AT        1:1  16 2048  B C            816SPU ADD-ON BOARD       
PERCEPTIVE SOLS.  HYPERSTORE1600 ISA-PROPRIETARY           AT        1:1                FULL      20MB CACHE(MAX) MAIN BRD. 
PERCEPTIVE SOLS.  SCSI ADAPTER   PRO.-SCSI        7HD      AT        1:1                          1600 ADD-ON BOARD (4 MAX) 
 
 
 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 4
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
PERFORM. TECHS.   PT-SCS350      SCSI-FLOPPY          4FD  NONE                      C            DOES NOT PLUG-IN          
PERSTOR SYSTEMS   PS180-16F      ISA-ST412*       2HD 2FD  AT        1:1  15 2048  B    FULL AT   UTILIZES ADRT RECORDING   
PERSTOR SYSTEMS   PS180-8        ISA-ST412*       2HD      XT,AT     1:1           B    FULL XT   UTILIZES ADRT RECORDING   
PERSTOR SYSTEMS   PS200-16F      ISA-ST412*       2HD 2FD  AT        1:1  15 2048  B    FULL AT   UTILIZES ADRT RECORDING   
PERSTOR SYSTEMS   PS200-8        ISA-ST412*       2HD      XT,AT     1:1           B    FULL XT   UTILIZES ADRT RECORDING   
RANCHO TECHNOLOGY RT-10-AT       ISA-SCSI         7HD      AT                           FULL XT   HOST ADAPTER              
RANCHO TECHNOLOGY RT-10-XT       ISA-SCSI         7HD      XT,AT                        1/2  XT   HOST ADAPTER              
RANCHO TECHNOLOGY RT-100-XT      ISA-SCSI         7HD 4FD  XT,AT                        1/2  XT   HOST ADAPTER              
RANCHO TECHNOLOGY RT-1000-XT     ISA-SCSI         7HD 4FD  XT,AT                        1/2  XT   HOST ADAPTER              
S.O.T.A.          FLOPPY I/O +   ISA-FLOPPY           4FD  PC,XT                        1/2  XT   2-S, 2-P PORTS            
SCIEN. MICROSYS.  OMTI 510HAX    ISA-SCSI         7HD      PC,XT,AT                               HOST ADAPTER              
SCIEN. MICROSYS.  OMTI 512-HA3   ISA-SCSI (OCS)                                                   HOST ADAPTER              
SCIEN. MICROSYS.  OMTI 512-HA7   ISA-SCSI         7HD                                             HOST ADAPTER              
SCIEN. MICROSYS.  OMTI 5520A     ISA-ST412(MFM)   2HD      XT                                                               
SCIEN. MICROSYS.  OMTI 5526      ISA-ST412(MFM)   2HD      XT                                                               
SCIEN. MICROSYS.  OMTI 5527A     ISA-ST412(RLL)   2HD      XT                                                               
SCIEN. MICROSYS.  OMTI 6510      ISA-ESDI         2HD      XT                                                               
SCIEN. MICROSYS.  OMTI 8120      ISA-ST412(MFM)   2HD      AT                           1/2                                 
SCIEN. MICROSYS.  OMTI 8127      ISA-ST412(RLL)   2HD      AT                           1/2                                 
SCIEN. MICROSYS.  OMTI 8620      ISA-ESDI         2HD 2FD  AT        1:1                                                    
SCIEN. MICROSYS.  OMTI 8627      ISA-ESDI         2HD 2FD  AT        1:1                                                    
SCIEN. MICROSYS.  OMTI 8627A     ISA-ST412(RLL)   2HD 2FD  AT                                                               
SEAGATE TECH.     ST-01          ISA-SCSI         2HD      PC,XT,AT                B    1/2  XT   HOST ADAPTER              
SEAGATE TECH.     ST-02          ISA-SCSI         2HD 2FD  PC,XT,AT                B    1/2  XT   HOST ADAPTER              
SEAGATE TECH.     ST-11M         ISA-ST412(MFM)   2HD      PC,XT,AT                     1/2  XT                             
SEAGATE TECH.     ST-11R         ISA-ST412(RLL)   2HD      PC,XT,AT                     1/2  XT                             
SILICON VALLEY    ADP20          ISA-IDE(AT)      2HD 2FD  AT                           1/2  XT                             
SILICON VALLEY    CADP60         ISA-IDE(AT)      2HD 4FD  AT                           1/2  XT                             
SILICON VALLEY    GOLD-MINE 1100 ISA-SCSI         7HD 2FD  PC,XT,AT                     1/2  XT   HOST ADAPTER              
STORAGE RESEARCH  SR-9           ISA-SCSI         7HD 2FD  PC,XT,AT                B    1/2  XT   HOST ADAPTER, 1 SPEED FDs 
WESTERN DIGITAL   ADSI-D215S     SCSI-ESDI        2HD      NONE                                   DOES NOT PLUG IN          
WESTERN DIGITAL   WD1001-WAH     CPU-ST412(MFM)   2HD      NONE                                   DOES NOT PLUG-IN          
WESTERN DIGITAL   WD1002-27X     ISA-ST412(RLL)   2HD      PC,XT,AT       16 1024  B C  1/2  XT   PWR. CONN. ON BOARD       
WESTERN DIGITAL   WD1002A-27X    ISA-ST412(RLL)   2HD      PC,XT,AT       16 1024  B    1/2  XT   NO JUMPERS                
WESTERN DIGITAL   WD1002A-FOX    ISA-FLOPPY           *FD  XT,AT                   *    1/2  XT   *OP#1=2F,#2=4F,#4=#2&BIOS 
WESTERN DIGITAL   WD1002A-WX1    ISA-ST412(MFM)   2HD      PC,XT,AT       16 1024  B C  1/2  XT   PWR. CONN. ON BOARD       
WESTERN DIGITAL   WD1002S-SHD    SASI-ST412(MFM)  2HD      NONE                                   DOES NOT PLUG IN          
WESTERN DIGITAL   WD1003-RA2     ISA-ST412(RLL)   2HD 2FD  AT        3:1  16 2048       FULL AT                             
WESTERN DIGITAL   WD1003-RAH     ISA-ST412(RLL)   2HD      AT        3:1  16 2048       FULL AT   W/ COMPAQ SETTING         
WESTERN DIGITAL   WD1003-WA2     ISA-ST412(MFM)   2HD 2FD  AT        3:1  16 2048       FULL AT                             
WESTERN DIGITAL   WD1003-WAH     ISA-ST412(MFM)   2HD      AT        3:1  16 2048                 W/ COMPAQ SETTING         
 
 
 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 5
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
WESTERN DIGITAL   WD1003A-RA2    ISA-ST412(RLL)   2HD 2FD  AT        2:1                     XT                             
WESTERN DIGITAL   WD1003A-SCS    SCSI-ST412(MFM)  2HD      NONE                                   DOES NOT PLUG IN          
WESTERN DIGITAL   WD1003A-WA2    ISA-ST412(MFM)   2HD 2FD  AT        3:1  16 2048       FULL XT                             
WESTERN DIGITAL   WD1003S-RA2    ISA-ST412(RLL)   2HD 2FD  AT        2:1                3/4                                 
WESTERN DIGITAL   WD1003S-RAH    ISA-ST412(RLL)   2HD      AT        2:1                3/4       W/ COMPAQ SETTING         
WESTERN DIGITAL   WD1003S-WA2    ISA-ST412(MFM)   2HD 2FD  AT        2:1                3/4                                 
WESTERN DIGITAL   WD1003S-WAH    ISA-ST412(MFM)   2HD      AT        2:1                3/4       W/ COMPAQ SETTING         
WESTERN DIGITAL   WD1003V-MM1    ISA-ST412(MFM)   2HD      AT        2:1  16 2048       3/4  XT                             
WESTERN DIGITAL   WD1003V-MM2    ISA-ST412(MFM)   2HD 2FD  AT        2:1  16 2048       3/4  XT                             
WESTERN DIGITAL   WD1003V-SR1    ISA-ST412(RLL)   2HD      AT        2:1  16 2048  *    3/4  XT   *BIOS OPTION              
WESTERN DIGITAL   WD1003V-SR2    ISA-ST412(RLL)   2HD 2FD  AT        2:1  16 2048  *    3/4  XT   *BIOS OPTION              
WESTERN DIGITAL   WD1004-27X     ISA-ST412(RLL)   2HD      XT,AT          16 1024  B C  1/2  XT   PWR. CONN. ON BOARD       
WESTERN DIGITAL   WD1004A-27X    ISA-ST412(RLL)   2HD      PC,XT          16 1024  B    1/2  XT                             
WESTERN DIGITAL   WD1004A-WX1    ISA-ST412(MFM)   2HD      PC,XT          16 1024  B C  1/2  XT   PWR. CONN. ON BOARD       
WESTERN DIGITAL   WD1005-WAH     ISA-ESDI         2HD      AT        2:1                     XT                             
WESTERN DIGITAL   WD1006-RA2     ISA-ST412(RLL)   2HD 2FD  AT        1:1                     XT                             
WESTERN DIGITAL   WD1006-RAH     ISA-ST412(RLL)   2HD      AT        1:1  16 2048  *         XT   W/ COMPAQ SETTING, *OPT.  
WESTERN DIGITAL   WD1006-WA2     ISA-ST412(MFM)   2HD 2FD  AT        1:1                     XT                             
WESTERN DIGITAL   WD1006-WAH     ISA-ST412(MFM)   2HD      AT        1:1  16 2048            XT   W/ COMPAQ SETTING         
WESTERN DIGITAL   WD1006V-MC1    MCA-ST412(MFM)   2HD      MCA       1:1                                                    
WESTERN DIGITAL   WD1006V-MCR    MCA-ST412(RLL)   2HD      MCA       1:1  16 2048       FULL MC                             
WESTERN DIGITAL   WD1006V-MM1    ISA-ST412(MFM)   2HD      AT        1:1  16 2048       3/4  XT   CACHE                     
WESTERN DIGITAL   WD1006V-MM2    ISA-ST412(MFM)   2HD 2FD  AT        1:1  16 2048       3/4  XT   CACHE                     
WESTERN DIGITAL   WD1006V-SR1    ISA-ST412(RLL)   2HD      AT        1:1  16 2048  *    3/4  XT   *BIOS OPTION, CACHE       
WESTERN DIGITAL   WD1006V-SR2    ISA-ST412(RLL)   2HD 2FD  AT        1:1  16 2048  *    3/4  XT   *BIOS OPTION, CACHE       
WESTERN DIGITAL   WD1007-WA2     ISA-ESDI         2HD 2FD  AT        1:1                3/4                                 
WESTERN DIGITAL   WD1007-WAH     ISA-ESDI         2HD      AT        1:1                3/4                                 
WESTERN DIGITAL   WD1007A-WA2    ISA-ESDI         2HD 2FD  AT        1:1           *    3/4  XT   *BIOS OPTION, 10 Mbps     
WESTERN DIGITAL   WD1007A-WA4    ISA-ESDI         2HD 2FD  AT        1:1           *         XT   *BIOS OPTION, CACHE,1P,1S 
WESTERN DIGITAL   WD1007A-WAH    ISA-ESDI         2HD      AT        1:1           *    3/4  XT   *BIOS OPTION, 10 mbps     
WESTERN DIGITAL   WD1007V-MC1    MCA-ESDI         2HD      MCA       1:1                FULL MC   15 Mbps                   
WESTERN DIGITAL   WD1007V-SE1    ISA-ESDI         2HD      AT        1:1           *    3/4  XT   *OPTION, CACHE, 15 Mbps   
WESTERN DIGITAL   WD1007V-SE2    ISA-ESDI         2HD 2FD  AT        1:1           *    3/4  XT   *OPTION, CACHE, 15 Mbps   
WESTERN DIGITAL   WD1009V-MM1    ISA-ESDI         2HD      AT        1:1  16 2048                 20 Mbps                   
WESTERN DIGITAL   WD1009V-MM2    ISA-ESDI         2HD 2FD  AT        1:1  16 2048                 20 Mbps                   
WESTERN DIGITAL   WD7000-ASC     ISA-SCSI         7HD 2FD  AT        1:1           B C  FULL AT   DOS ONLY                  
WESTERN DIGITAL   WD7000-FASST2  ISA-SCSI         7HD 2FD  AT        1:1           B C  FULL AT   DOS,UNIX,NOVELL DRIVERS   
WESTERN DIGITAL   WD7000MX-FASST MCA-SCSI         7HD      MCA                          FULL MC   HOST ADAPTER (WD7000-MSC) 
WESTERN DIGITAL   WDAT140R       ISA-IDE(AT)      2HD      AT                                     HOST ADAPTER              
WESTERN DIGITAL   WDAT240R       ISA-IDE(AT)      1HD 2FD  AT                                     HOST ADAPTER              
WESTERN DIGITAL   WDAT440R       ISA-IDE(AT)      1HD 2FD  AT                                     HOST ADPT, 1-PAR, 2-SER.  
 
 
 
 
                                               DISK DRIVE CONTROLLER LISTING  V3.0
                                                   compiled by F. Robert Falbo
Feb. 17, 1990                                                                                                           Page 6
 
                                   INTERFACES     DRIVES     BUS          ©-MAX-ª    C  ©-SIZE-ª                            
MANUFACTURER       MODEL NUMBER     INVOLVED      HDs FDs  SUPPORT   INT  HD SECT  B R  LGN. HGT.    COMMENTS               
----------------------------------------------------------------------------------------------------------------------------
 
WESTERN DIGITAL   WDATXT-FASST   ISA-SCSI         7HD 2FD  XT,AT                        1/2  XT   HOST ADAPTER              
WESTERN DIGITAL   WDSPEEDKIT     ISA-ST412(MFM)   2HD 2FD  AT        1:1                3/4  XT   CACHE                     
WESTERN DIGITAL   WDXT-GEN       ISA-ST412(MFM)   2HD      PC,XT          8  1024  B    1/2  XT   NO JUMPERS                
WESTERN DIGITAL   WDXT-GEN2      ISA-ST412(MFM)   2HD      XT,AT          8  1024  B    1/2  XT                             
WESTERN DIGITAL   WDXT140R       ISA-IDE(XT)      1HD      XT                                XT   HOST ADAPTER              
WESTERN DIGITAL   WDXT150R       ISA-IDE(XT)      1HD      XT                                XT   HOST ADAPTER, W/PWR CONN. 
XEBEC             S1210          ISA-ST412(MFM)   2HD      PC,XT                                                            
XEBEC             S1410          ISA-ST412(MFM)   2HD      PC,XT                                                            
XEBEC             S1412          ISA-ST412(MFM)   2HD 2FD  PC,XT                                                            
 
ÉÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍ»
º  DRIVE CONTROLLER REFERENCE LISTING  VER. 3.0      ABBREVIATIONS    º
º                                                                     º
º  FDs ....... FLOPPY DISKS             B ........ BIOS ON CARD(?)    º
º  HDs ....... HARD DISKS               CR ....... CO-RESIDENT(?)     º
º  INT ....... INTERLEAVE               LGN ...... LENGTH OF CARD     º
º  Ú HD ...... MAX. HEADS SUPPORTED     HGT ...... HEIGHT OF CARD     º
º  À SECT .... MAX. SECTORS SUPPORTED                                 º
ÇÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¶
º  c1990 F.ROBERT FALBO        ¯¯¯ LIMITED RIGHTS RESERVED ®®®        º
ÇÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄÄ¶
º  The user of this information is granted permission to transmit it  º
º  Electronically with the restrictions that it not be altered in     º
º  regard to content or credit.  The Author may be reached at KADET   º
º  PcBoard (315)245-3815, or ALTERNATE ESCAPE PcBoard (315)336-1613.  º
ÈÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍÍ¼
 
          
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
