#  EPSON LQ Driver Version 1.1
#  Copyright Douglas P. Webb 1993, All rights reserved.

#  This is a comment. The # at the beginning of the line makes it so.
#  No line which is not a comment may exceed 80 characters.

#  A line which consists only of the string CRLF will generate a
#    carriage return/linefeed in the output to the printer

#  Anything starting with ~ is a variable unless it's ~~
#  Predefined variables are:
#     ~R   which is the current row (line number)
#     ~C   which is the current column


[DEFINES]


# Turn off possible compressed/expanded/double strike printing
# Use Near Letter Quality
# If you find NLQ slows things down too much remove the x at
#    the end of the line after preamble
[PREAMBLE]
Hx


#Formfeed
#If you don't want a formfeed at the end of every page erase the  after
#  postamble
[POSTAMBLE]



# Set double strike
[BOLD]
G


# Turn off double strike
[NORMAL]
H


[PRELINE]


#default is carriage return/linefeed
[POSTLINE]


[FORMFEED]



[REPLACE]


# Number of lines of text that should appear on a page
[LINES/PAGE]
62