#  Deskjet 500 Driver Version 1.1
#  Copyright Douglas P. Webb 1993, All rights reserved.

#  This is a comment. The # at the beginning of the line makes it so.
#  No line which is not a comment may exceed 80 characters.

#  A line which consists only of the string CRLF will generate a
#    carriage return/linefeed in the output to the printer

#  Anything starting with ~ is a variable unless it's ~~
#  Predefined variables are:
#     ~R   which is the current row (line number)
#     ~C   which is the current column


# No Defines required for HP Deskjet
[DEFINES]


#Reset the printer
#Select Normal Courier Font
#Set line spacing and number of lines per page. (8 lines/inch & 60/page)
#Set Default Left/Right Margins
[PREAMBLE]
E
&l0O(8U(s0p10h12v0s0b3t2Q
&l8D
&a3l80M



[POSTAMBLE]
&l0H

#Select Bold font.
[BOLD]
&l0O(8U(s0p10h12v0s3b3t2Q

#Select Normal font.
[NORMAL]
&l0O(8U(s0p10h12v0s0b3t2Q


# No preline treatment required for HP Deskjet 500 printer
[PRELINE]


#default is carriage return/linefeed
[POSTLINE]


[FORMFEED]
&l0H


[REPLACE]


# Number of lines of text that should appear on a page
[LINES/PAGE]
60